

Left Opening

3) Assemble the perimetral gasket again

1. Remove perimetral gasket

2) Fix frame/counterframe with self-drilling screws

Personal Door Fixing



Personal Door Detail